! Temperature Flight Planning Table temper19.rdf  08-Jan-2008

Temperature Flight Planning Table Version   (-)     = 1.13-20080108

Number of Cooling Zones                     (-)     =    4 ! Nz
Baseline Antenna Duty Cycle                 (-)     = 100.0 ! % Max heater pwr
Minimum Antenna Duty Cycle                  (-)     = 100.0 ! % Max heater pwr

! It is assumed that the cooling zones are numbered from 1, ..., Nz.
! One block of parameters is defined for each cooling zone.
! The value of Nzone is embedded within each RDF keyword.

! Zone 1 is the forced air cooling duct that cools the JBOD 
Zone 1 Type                                 (-) =      0 ! 0 = disabled - ZoneType = 2 = electronics to enable
Zone 1 Antenna Number                       (-) =      0 ! Nantenna
Zone 1 Control Temperature Maximum          (-) =  32815 ! Thi, units 0.01K, +55 C   [Green = +25 - +40]
Zone 1 Control Temperature Minimum          (-) =  27315 ! Tlo, units 0.01K, 0 C
Zone 1 Upper Red Region Width               (-) =   1000 ! dTru, units 0.01K, upper red > +45
Zone 1 Lower Red Region Width               (-) =   2000 ! dTrl, units 0.01K, lower red < +20 
Zone 1 Upper Yellow Region Width            (-) =    500 ! dTyu, units 0.01K, upper ylw +40 - +45
Zone 1 Lower Yellow Region Width            (-) =    500 ! dTyl, units 0.01K, lower ylw +20 - +25
Zone 1 Inlet Air Temperature Sensor Count   (-) =      2 ! Nair
Zone 1 Inlet Air Temperature Sensor 1       (-) =      1 ! Nambient
Zone 1 Inlet Air Temperature Sensor 2       (-) =      2 
Zone 1 Control Temperature Sensor Count     (-) =      1 ! Ncont
Zone 1 Control Temperature Sensor 1         (-) =      5 ! Ncontrol JBOD
Zone 1 Control Temperature Sensor 1 Heater  (-) =      0 ! Nconhtr
Zone 1 Monitor Temperature Sensor Count     (-) =      1 ! Nmon
Zone 1 Monitor Temperature Sensor 1         (-) =      4 ! Nmonitor JBOD
Zone 1 Monitor Temperature Sensor 1 Heater  (-) =      0 ! Nmonhtr
Zone 1 Monitor Temperature Sensor 1 Maximum (-) =  32815 ! Tmax, units 0.01K, +55 C
Zone 1 Monitor Temperature Sensor 1 Minimum (-) =  27315 ! Tmin, units 0.01K, 0 C

! Zone 2 contains all the electronics except the JBOD 
Zone 2 Type                                 (-) =      2 ! ZoneType = 2 = electronics, = 0 = disable
Zone 2 Antenna Number                       (-) =      0 ! Nantenna
Zone 2 Control Temperature Maximum          (-) =  31815 ! Thi, +45 C  [Green = +25 - +35]
Zone 2 Control Temperature Minimum          (-) =  28815 ! Tlo, +15 C
Zone 2 Upper Red Region Width               (-) =    500 ! dTru, upper red > +40
Zone 2 Lower Red Region Width               (-) =    500 ! dTrl, lower red < +20
Zone 2 Upper Yellow Region Width            (-) =    500 ! dTyu, upper ylw +35 - +40
Zone 2 Lower Yellow Region Width            (-) =    500 ! dTyl, lower ylw +20 - +25
Zone 2 Inlet Air Temperature Sensor Count   (-) =      2 ! Nair
Zone 2 Inlet Air Temperature Sensor 1       (-) =      8 ! Nambient
Zone 2 Inlet Air Temperature Sensor 2       (-) =      9
Zone 2 Control Temperature Sensor Count     (-) =      4 ! Ncont
Zone 2 Control Temperature Sensor 1         (-) =     11 ! Ncontrol Digital VME
Zone 2 Control Temperature Sensor 1 Heater  (-) =      1 ! Nconhtr Heater #1 to enable
Zone 2 Control Temperature Sensor 2         (-) =     32 ! PDU
Zone 2 Control Temperature Sensor 2 Heater  (-) =      6
Zone 2 Control Temperature Sensor 3         (-) =     13 ! RF VME
Zone 2 Control Temperature Sensor 3 Heater  (-) =      2 ! Heater #2 to enable
Zone 2 Control Temperature Sensor 4         (-) =     16 ! DGPS 
Zone 2 Control Temperature Sensor 4 Heater  (-) =      3
Zone 2 Monitor Temperature Sensor Count     (-) =      4 ! Nmon
Zone 2 Monitor Temperature Sensor 1         (-) =     12 ! Nmonitor Digital VME
Zone 2 Monitor Temperature Sensor 1 Heater  (-) =      1 ! Nmonhtr Heater #1 to enable
Zone 2 Monitor Temperature Sensor 1 Maximum (-) =  31815 ! Tmax, +45 C 
Zone 2 Monitor Temperature Sensor 1 Minimum (-) =  25815 ! Tmin, -15 C
Zone 2 Monitor Temperature Sensor 2         (-) =     31 ! PDU
Zone 2 Monitor Temperature Sensor 2 Heater  (-) =      6
Zone 2 Monitor Temperature Sensor 2 Maximum (-) =  31815 ! Tmax, +45 C
Zone 2 Monitor Temperature Sensor 2 Minimum (-) =  25815 ! Tmin, -15 C
Zone 2 Monitor Temperature Sensor 3         (-) =     14 ! RF VME
Zone 2 Monitor Temperature Sensor 3 Heater  (-) =      2 ! Heater #2 to enable
Zone 2 Monitor Temperature Sensor 3 Maximum (-) =  31315 ! Tmax, +40 C
Zone 2 Monitor Temperature Sensor 3 Minimum (-) =  25815 ! Tmin, -15 C
Zone 2 Monitor Temperature Sensor 4         (-) =     15 ! DGPS
Zone 2 Monitor Temperature Sensor 4 Heater  (-) =      3
Zone 2 Monitor Temperature Sensor 4 Maximum (-) =  31815 ! Tmax, +45 C
Zone 2 Monitor Temperature Sensor 4 Minimum (-) =  26815 ! Tmin, -5 C

! Zone 3 is the L-band antenna cooling duct 
Zone 3 Type                                 (-) =  1     ! ZoneType = 1 = antenna
Zone 3 Antenna Number                       (-) =  1     ! antenna #1
Zone 3 Control Temperature Maximum          (-) =  30815 ! Thi, +35 C [Green -5 - +5]
Zone 3 Control Temperature Minimum          (-) =  23815 ! Tlo, -35 C
Zone 3 Upper Red Region Width               (-) =    500 ! dTru, upper red > +30 
Zone 3 Lower Red Region Width               (-) =    500 ! dTrl, lower red < -30
Zone 3 Upper Yellow Region Width            (-) =   2500 ! dTyu, upper ylw +5 - +30
Zone 3 Lower Yellow Region Width            (-) =   2500 ! dTyl, lower ylw -30 - -5
Zone 3 Inlet Air Temperature Sensor Count   (-) =      0 ! Nair
Zone 3 Control Temperature Sensor Count     (-) =      3 ! Ncont
Zone 3 Control Temperature Sensor 1         (-) =     22
Zone 3 Control Temperature Sensor 1 Heater  (-) =      9
Zone 3 Control Temperature Sensor 2         (-) =     23
Zone 3 Control Temperature Sensor 2 Heater  (-) =      9
Zone 3 Control Temperature Sensor 3         (-) =     24
Zone 3 Control Temperature Sensor 3 Heater  (-) =      9
Zone 3 Monitor Temperature Sensor Count     (-) =      3 ! Nmon
Zone 3 Monitor Temperature Sensor 1         (-) =     22
Zone 3 Monitor Temperature Sensor 1 Heater  (-) =      9
Zone 3 Monitor Temperature Sensor 1 Maximum (-) =  30815 ! Tmax, +35 C
Zone 3 Monitor Temperature Sensor 1 Minimum (-) =  23815 ! Tmin, -35 C
Zone 3 Monitor Temperature Sensor 2         (-) =     23
Zone 3 Monitor Temperature Sensor 2 Heater  (-) =      9
Zone 3 Monitor Temperature Sensor 2 Maximum (-) =  30815 ! Tmax, +35 C
Zone 3 Monitor Temperature Sensor 2 Minimum (-) =  23815 ! Tmin, -35 C
Zone 3 Monitor Temperature Sensor 3         (-) =     24
Zone 3 Monitor Temperature Sensor 3 Heater  (-) =      9
Zone 3 Monitor Temperature Sensor 3 Maximum (-) =  30815 ! Tmax, +35 C
Zone 3 Monitor Temperature Sensor 3 Minimum (-) =  23815 ! Tmin, -35 C

! Zone 4 is used for electronics not connected to any cooling duct
Zone 4 Type                                 (-) =      2 ! ZoneType = 2 = electronics, = 0 = disable
Zone 4 Antenna Number                       (-) =      0 ! Nantenna
Zone 4 Control Temperature Maximum          (-) =  31815 ! Thi - not used
Zone 4 Control Temperature Minimum          (-) =  27815 ! Tlo - not used
Zone 4 Upper Red Region Width               (-) =   1000 ! dTru - not used
Zone 4 Lower Red Region Width               (-) =    500 ! dTrl - not used
Zone 4 Upper Yellow Region Width            (-) =    500 ! dTyu - not used
Zone 4 Lower Yellow Region Width            (-) =    500 ! dTyl - not used
Zone 4 Inlet Air Temperature Sensor Count   (-) =      0 ! Nair
Zone 4 Control Temperature Sensor Count     (-) =      0 ! Ncont
Zone 4 Monitor Temperature Sensor Count     (-) =      1 ! Nmon
Zone 4 Monitor Temperature Sensor 1         (-) =     19 ! Battery 
Zone 4 Monitor Temperature Sensor 1 Heater  (-) =      5
Zone 4 Monitor Temperature Sensor 1 Maximum (-) =  30315 ! Tmax, +30 C (Heater turns off.)
Zone 4 Monitor Temperature Sensor 1 Minimum (-) =  26315 ! Tmin, -10 C (Heater turns on.)

! End of table
