! ROW CTU COMMAND TABLE

ROW CTU Command Table Version       = 1.00-20060501

flight_id                = 10000   ! Flight ID
plan_id                  =  1232   ! Flight Plan ID
flight_line_id           = 01200   ! Flight ID

data_take_type           =    17   ! data take
caltone_routing_select   =     2   ! RFN=1, ASN=2

antenna_select           =     1   ! 1=1, 2=2, 1&2=3
tx_pol_select            =     3   ! H=1, V=2, or Alt H&V=3
rx_array_select          =     1   ! Full=1, Split H=2, Split V=3, Split H&V=4
rx_buffer_select         =     3   !  1=1, 2=2, 1&2=3

tx_pulse_length          =    40   ! TX Pulse Length

beam_steering_mode       =     2   ! 1 = BODY FIX, 2 = TRACK FIX
scan_angle_count         =     1   ! Scan Angle Count
steering_angle_1         =     0   ! Steering Angle 1   10*degrees   
steering_angle_2         =     0   ! Steering Angle 2   10*degrees   
steering_angle_3         =     0   ! Steering Angle 3   10*degrees   

optimum_steering_angle   =   516   ! Optimum Steering Angle 10*degrees
steering_update_threshold=     5   ! Steering Update Threshold 10*degrees
steering_update_rate     =     5   ! Steering Update Rate (# of 50-Hz cycles between updates) 
track_heading            =    12   ! Track Heading degrees

pri_min                  =  1876   ! Microseconds, 1000 to 10000, steps of 2   
pri_max                  =  5000   ! Microseconds, 1000 to 10000, steps of 2   
targeted_feet_per_pulse  =    20   ! Targeted Feet/Pulse (10*feet_per_pulse)   

dwp_start                =   114   ! Microseconds, 20 to 510, steps of 2   
dwp_duration             =   150   ! Microseconds, 50 to 150, steps of 10   

bfpq_comp_fact           =     8   ! 0 to 12 BFPQ Compression Ratio   
bfpq_comp_size           =     2   ! 0=none, 1=64, 2=128, 3=256 BFPQ Block Size   

ant_tx_enable            =     1   ! 0=no, 1=yes   
ant_rx_enable            =     1   ! 0=no, 1=yes   
sniffer_pulse_enable     =     1   ! 0=no, 1=yes   
cal_pulse_interval       =   255   ! Calibration Pulse Interval   

gain_rcvr_1_f1_m1        = 22   ! PRF 1 RCVR 1: 0 to 56, steps of 2   
gain_rcvr_2_f1_m1        = 14   ! PRF 1 RCVR 2: 0 to 56, steps of 2   
gain_rcvr_1_f1_m2        = 14   ! PRF 2 RCVR 1: 0 to 56, steps of 2   
gain_rcvr_2_f1_m2        = 22   ! PRF 2 RCVR 2: 0 to 56, steps of 2   
gain_rcvr_1_f1_m3        = 0   ! PRF 3 RCVR 1: 0 to 56, steps of 2   
gain_rcvr_2_f1_m3        = 0   ! PRF 3 RCVR 2: 0 to 56, steps of 2   
gain_rcvr_1_f1_m4        = 0   ! PRF 4 RCVR 1: 0 to 56, steps of 2   
gain_rcvr_2_f1_m4        = 0   ! PRF 4 RCVR 2: 0 to 56, steps of 2   
gain_rcvr_1_f1_m5        = 0   ! PRF 5 RCVR 1: 0 to 56, steps of 2   
gain_rcvr_2_f1_m5        = 0   ! PRF 5 RCVR 2: 0 to 56, steps of 2   
gain_rcvr_1_f1_m6        = 0   ! PRF 6 RCVR 1: 0 to 56, steps of 2   
gain_rcvr_2_f1_m6        = 0   ! PRF 6 RCVR 2: 0 to 56, steps of 2   
agc_flag                 = 0   ! 1=AGC on, 0=AGC off   

awg_file_name            = 00123201.awg   ! AWG File Name   
site_name                =                     sabine_01200   ! Site Name   
